

X10QRH+ Release note:	 
CPU µ-code	Firmware	 
CPUID	Family	Stepping	Rev.	VGA: 0.96.00	 
306F0	HW-EP	A0	17	Intel® SATA RAID Legacy: 4.5.1012	
306F1	HW-EP	B0	14	Intel® sSATA RAID Legacy: 4.5.1012	
306F2	HW-EP	C0/C1/M1	38	Intel® SATA RAID UEFI: 4.5.1012	
406F0	BW-EP	A0/A1/L0	14	Intel® sSATA RAID UEFI: 4.5.1012	
406F1	BW-EP	B0/M0/R0	1B	Intel® 1Gb LAN UEFI driver: 5.0.12	
	Intel® 10Gb LAN UEFI driver: 3.4.12	
	TXT/ACM: Grantley 3.0.5 20160315	
	Intel® ME: 3.1.3.36	
	Intel® RC: 3.5.0	
BIOS Feature	Out of Band Flash BIOS	Out of Band Update Setting	Out of Band  Change SMBIOS	In Band Flash BIOS	In Band Update Setting	In Band Change SMBIOS	In Band SMI E7h Supported
Supported	Yes	Yes	Yes	Yes	Yes	Yes	Yes
	
BIOS: X10QRH6.614 
	Revision: 2.0
	Release Date: 6/14/2016
	
1.	Whole code upgrade to AMI code base of refresh rev. 22.
Description: Whole code base upgrade for Broadwell processor.
Validation:  Notice only
2.	Update Intel® RSTe to ver. 4.5.0.1012.
Description: Routine update.
Validation: Go to SATA ROM config.(legacy) or RSTe SATA controller option of BIOS setup menu to check version.
3.	Update R.C. to ver. 3.5.0.
Description: Up to date version. May improve performance for some benchmarks.
Validation: Notice only.
4.	Update ME to ver. 3.1.3.36.
Description: Up to date version.
Validation: Dependency of RC 3.5.0.
5.	Update CPUµcode of Broadwell B0, M0 and R0 to ver. 1B.
Description: Up to date version.
Validation: Dependency of RC 3.4.0 and later one.
6.	Support TPM 2.0
Description: As title.
Validation: Refer to issue# of super-eco.
7.	Support DDR4 3DS RDIMM.
Description: As title.
Validation: Make sure system works properly with DDR4 3DS DIMM.
8.	Add onboard LAN2, LAN3 and LAN4 OPROM setup options.
Description: As title.
Validation: Check BIOS setup menu.
9.	Add workaround of Intel OMNI Path 100Gb LAN card.
Description: For this card got problem in GEN3 during POST.
Validation: Make sure this card is working properly in OS.
10.	Ad “OUx Non-Posted Fetch” setup options.
Description: As title.
Validation: Check BIOS setup menu.
11.	Fix no 10Gb and 40Gb LAN card temperature showed by IPMI.
Description: Implement IPMI OEM command 30 68 properly.
Validation: Make sure its temperature is showed by IPMI with an Intel 10Gb LAN.
12.	Correct NUMA length matrix when cluster-on-die(COD) is enabled.
Description: As title.
Validation: Enable COD and use numactl command to check with.
13.	Improve RAI D option ROM is invisible in some condition.
Description: Increase the delay of showing SATA and sSATA prompt message.
Validation: Validated by Chu L.(issue #63224 of super-eco)
14.	Improve Mellanox 100Gb LAN card low performance
Description: As title, problem is raised by customer.
Validation: Refer to issue #70738 of super-eco.
15.	Fix for TPM options no longer appear after disabling "Security Device Support".
Description: As title.
Validation: Disable “Security Device Support” and make sure TPM appears in next entering to setup menu.
16.	Patch for system may stop at POST code 61.
Description: Unknown CMOS-alarm-int at early boot time causes system stops.
Validation: Run reboot test more than 100 times.
17.	Fix some SUM test fail items.
a.	Number of PSU mismatch
Description: Incorrect PSU number in SUM report.
Validation: Run test case #223.
b.	Modify BIOS coding issue.
Description: Some system BIOS setup options cannot be modified by SUM
Validation: Run test case #220.
	
							
